{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":33,"n_cols":14,"rows_kept":33,"flags":["formulas_cached_only"]}
[null,"Frequency Codes for PSM600"]
[]
[]
[null,"United States ",null,"600 MHz Version (CE, FCC), 100mW",{"$nulls":4},"Nordic Countries",null,null,"20mW"]
[]
[null,null,"A","MHz",null,"B","MHz",null,null,"A","MHz",null,"B","MHz"]
[null,"HA =","LA",626.475,null,"LB",{"v":632.55,"d":"632.550"},null,"MH =","LR",{"v":808.6,"d":"808.600"},null,"LS",{"v":813.3,"d":"813.300"}]
[null,"HB =","LC",629.975,null,"LD",634.775,null,"MJ =","LT",{"v":811.6,"d":"811.600"},null,"LV",{"v":813.8,"d":"813.800"}]
[null,"HC =","LE",642.275,null,"LF",{"v":646.5,"d":"646.500"},null,"ML =","LL",{"v":801.1,"d":"801.100"},null,"LY",{"v":801.9,"d":"801.900"}]
[null,"HD =","LG",647.525,null,"LH",653.375,null,"MM =","LZ",{"v":817.2,"d":"817.200"},null,"RA",{"v":819.7,"d":"819.700"}]
[null,"HE =","LJ",{"v":655.25,"d":"655.250"},null,"LK",{"v":656.5,"d":"656.500"}]
[]
[]
[]
[null,"Germany",null,"800 MHZ Version (CE, BZT), 20mW",{"$nulls":4},"United Kingdom, Turkey",null,null,"10mW"]
[]
[null,null,"A","MHz",null,"B","MHz",null,null,"A","MHz",null,"B","MHz"]
[null,"MF =","LL",{"v":801.1,"d":"801.100"},null,"LM",{"v":802.55,"d":"802.550"},null,"KB =","RB",{"v":854.9,"d":"854.900"},null,"RC",856.175]
[null,"MG =","LN",{"v":805.05,"d":"805.050"},null,"LP",{"v":810.55,"d":"810.550"},null,"KC =","RD",{"v":856.95,"d":"856.950"},null,"RE",{"v":860.4,"d":"860.400"}]
[null,"MH =","LR",{"v":808.6,"d":"808.600"},null,"LS",{"v":813.3,"d":"813.300"},null,"KD =","RF",859.375,null,"RG",{"v":860.9,"d":"860.900"}]
[null,"MJ =","LT",{"v":811.6,"d":"811.600"},null,"LV",{"v":813.8,"d":"813.800"}]
[null,"MK =","LW",823.475,null,"LX",{"v":827.7,"d":"827.700"}]
[]
[{"$nulls":3},"alle Nutzergruppe 4",{"$nulls":5},"Nutzer 4","Nutzer 3"]
[]
[]
[null,"Sweden",null,null,"20 mW",{"$nulls":3},"Netherlands",null,null,"100mW"]
[]
[null,null,"A","MHz",null,"B","MHz",null,null,"A","MHz",null,"B","MHz"]
[null,"MF =","LL",{"v":801.1,"d":"801.100"},null,"LM",{"v":802.55,"d":"802.550"},null,"HG =","NF",{"v":630.5,"d":"630.500"},null,"NG",{"v":633.25,"d":"633.250"}]
[null,"MG =","LN",{"v":805.05,"d":"805.050"},null,"LP",{"v":810.55,"d":"810.550"},null,"HH =","NN",634.875,null,"NS",636.875]
[null,"MH =","LR",{"v":808.6,"d":"808.600"},null,"LS",{"v":813.3,"d":"813.300"}]
[null,"MJ =","LT",{"v":811.6,"d":"811.600"},null,"LV",{"v":813.8,"d":"813.800"}]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}