{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["K5E","T1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"K5E","index":0,"n_rows":13,"n_cols":11,"rows_kept":13,"merged":[[0,0,0,10]],"flags":["formulas_cached_only"]}
["PGX - K5E: 606 - 630 MHz"]
[]
["CHAN","Ch 1 - 9","Ch 11-19","Ch 21-29","Ch 31-39","Ch 41-49","Ch 51-59","Ch 61-69","Ch 71-79","Ch 81-89","Ch 91-99"]
[1,{"v":606.35,"d":"606.350"},606.675,606.125,{"v":606.25,"d":"606.250"},{"v":614.55,"d":"614.550"},{"v":614.2,"d":"614.200"},{"v":622.2,"d":"622.200"},{"v":615.25,"d":"615.250"},616.775,{"v":615,"d":"615.000"}]
[2,{"v":607.65,"d":"607.650"},607.775,{"v":607.3,"d":"607.300"},607.375,{"v":615.75,"d":"615.750"},{"v":615.8,"d":"615.800"},{"v":623.8,"d":"623.800"},{"v":616.5,"d":"616.500"},618.225,616.225]
[3,{"v":609.75,"d":"609.750"},609.175,{"v":609.25,"d":"609.250"},608.875,{"v":617.55,"d":"617.550"},{"v":616.9,"d":"616.900"},{"v":624.9,"d":"624.900"},{"v":619.75,"d":"619.750"},{"v":620.5,"d":"620.500"},618.775]
[4,{"v":610.85,"d":"610.850"},610.875,{"v":610.5,"d":"610.500"},{"v":610.95,"d":"610.950"},{"v":618.85,"d":"618.850"},618.475,626.475,{"v":623.5,"d":"623.500"},{"v":621.7,"d":"621.700"},{"v":620.7,"d":"620.700"}]
[5,612.425,{"v":612.05,"d":"612.050"},{"v":613.1,"d":"613.100"},612.475,621.025,620.375,628.375,{"v":626.5,"d":"626.500"},{"v":625.5,"d":"625.500"},{"v":621.9,"d":"621.900"}]
[6,{"v":613.7,"d":"613.700"},613.575,{"v":615.25,"d":"615.250"},{"v":615.3,"d":"615.300"},{"v":622.65,"d":"622.650"},{"v":621.5,"d":"621.500"},{"v":629.5,"d":"629.500"},{"v":628.25,"d":"628.250"},626.975,626.025]
[7,null,null,{"v":616.4,"d":"616.400"},{"v":616.85,"d":"616.850"},623.775,{"$nulls":3},{"v":628.9,"d":"628.900"},{"v":628,"d":"628.000"}]
[8,null,null,{"v":618,"d":"618.000"},619.325,625.675,{"$nulls":4},{"v":629.1,"d":"629.100"}]
[9,null,null,{"v":620.4,"d":"620.400"},{"v":620.6,"d":"620.600"},626.825]
[null,"U.K. preferred:\nTV ch. 38\n606-614 MHz\nwith 125 kHz guard band\n(same as SLX-K3E group 10)","U.K. preferred:\nTV ch. 38\n606-614 MHz\nwith 125 kHz guard band\n(same as SLX-K3E group 11)","Full Range max. # of\ncompatible frequencies\n(same as SLX-K3E group 2)","Full Range max. # of\ncompatible frequencies\n(same as SLX-K3E group 3)","Full Range max. # of\ncompatible frequencies,\nCh. 38 excl.\n(same as SLX-K3E group 4)","European TV channel 39\noptimized\n614 - 622 MHz\n(same as SLX-K3E group 15)","European TV channel 40\noptimized\n622 - 630 MHz\n(same as SLX-K3E group 16)","France preferred:\nUser Group A\n614 - 630 MHz\n(same as SLX-K3E group 12)","France preferred:\nUser Group B\n614 - 630 MHz\n(same as SLX-K3E group 13)","France preferred:\nUser Group C\n614 - 630 MHz\n(same as SLX-K3E group 14)"]

{"sheet":"T1","index":1,"n_rows":13,"n_cols":11,"rows_kept":13,"merged":[[0,0,0,10]],"flags":["formulas_cached_only"]}
["PGX - T1: 846 - 865 MHz"]
[]
["CHAN","Ch 1 - 9","Ch 11-19","Ch 21-29","Ch 31-39","Ch 41-49","Ch 51-59","Ch 61-69","Ch 71-79","Ch 81-89","Ch 91-99"]
[1,{"v":847.5,"d":"847.500"},{"v":846.1,"d":"846.100"},{"v":863.2,"d":"863.200"},{"v":846.8,"d":"846.800"},{"v":854.2,"d":"854.200"},855.475,855.075,{"v":854.75,"d":"854.750"},{"v":854.75,"d":"854.750"},854.425]
[2,{"v":848.6,"d":"848.600"},{"v":847.35,"d":"847.350"},{"v":863.9,"d":"863.900"},848.425,{"v":855.3,"d":"855.300"},857.425,857.775,{"v":855.85,"d":"855.850"},{"v":855.85,"d":"855.850"},855.525]
[3,{"v":850.1,"d":"850.100"},{"v":849.4,"d":"849.400"},{"v":864.5,"d":"864.500"},850.425,{"v":856.7,"d":"856.700"},{"v":860.6,"d":"860.600"},860.725,{"v":857.25,"d":"857.250"},{"v":857.25,"d":"857.250"},{"v":857.4,"d":"857.400"}]
[4,{"v":852.1,"d":"852.100"},{"v":851.8,"d":"851.800"},null,852.875,{"v":857.8,"d":"857.800"},null,null,{"v":858.35,"d":"858.350"},{"v":858.35,"d":"858.350"},{"v":858.5,"d":"858.500"}]
[5,{"v":853.3,"d":"853.300"},{"v":853.2,"d":"853.200"},null,{"v":855.65,"d":"855.650"},859.675,null,null,860.225,860.225,{"v":859.9,"d":"859.900"}]
[6,{"v":855.1,"d":"855.100"},null,null,856.775,860.775,null,null,861.325,861.325,{"v":861,"d":"861.000"}]
[7,{"v":857.2,"d":"857.200"},null,null,859.725]
[8,{"v":858.65,"d":"858.650"},null,null,{"v":861.55,"d":"861.550"}]
[9,{"v":859.8,"d":"859.800"},null,null,{"v":864.8,"d":"864.800"}]
["Amount of Channels in one TV-Channel","Compatible setup for use with EUT-VR, -VS and -VT","Compatible setup for use with EUT-TW, -TX, -TY and -TZ","European harmonized band: optimized for 863 - 865 MHz","Full Range max. #  of compatible frequencies (same as SLX-S6, group 3)","BEL / TUR preferred:       opt. TV ch.69      854-862 MHz ","U.K. preferred: \"CH69 Co-ordinated\" SET 1","U.K. preferred: \"CH69 Co-ordinated\"  SET 3","U.K. preferred: \"Co-ordinated frequencies\"  INDOORS","U.K. preferred: \"Co-ordinated frequencies\"  OUTDOORS (option 1)","U.K. preferred: \"Co-ordinated frequencies\"  OUTDOORS (option 2)"]